Windows Driver Installer Setup Program
(For PL2303 HXD, SA, TA, TB, RA GC, GS, GT, GL, GE , GD, GR versions)
Installer version & Build date: 2.0.6 (2021-5-13)
Windows Vista/7/8.1/10 (32 & 64-bit) WDF WHQL Driver: v3.8.39.0 (01/08/2021) / v5.1.0.0 (05/13/2021)
   - Windows 10  Certified WHQL Driver (TH1 1507, TH2 1511, RS1 1607, RS2 1703, RS3 1709, RS4 1803,RS5 1809,19H1 1903,19H2 1909, 20H1 VB versions)
   - Windows Vista, 7, 8.1 Certified WHQL Driver 
   - Compatible with Windows Server 2016, Server2008, 2008R2, 2012, 2012R2, 2019
   - Auto-download driver via Windows Update (Windows 7, 8.1, 10)
Windows XP (32 & 64-bit) WDM Driver: v3.8.38.0 (12/01/2020)
    - Compatible with Windows 2000SP4 & Server2003

Windows XP (32 & 64-bit) WDM WHQL Driver: v5.0.8.1 (07/08/2019)
    - Windows XP Certified WHQL Driver  
    - Compatible with Windows 2000SP4 & Server2003

- Installer Language Support: English (default), Chinese (Traditional and Simplified), Japanese
- For Prolific USB VID_067B&PID_2303, PID_2304, PID_23A3, PID_23B3, PID_23C3,PID_23D3,PID_23E3,PID_23F3,PID_2323.
- Includes Certification Report, User Manual, Driver Release Notes, CheckChipVersion Tool
- Installer supports silent install (add "/s" parameter when running program)